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1.
True or False?  The weight-bearing capacity of a floor can normally be determined by 


a visual inspection of its surface.
       
True

       
False

2.
True or False? Good housekeeping practices can prevent many slips, trips and falls.
       
True

       
False

3.
True or False? Railings must be installed on all open-sided platforms and catwalks that 


are four feet or more off the ground, to help prevent falls.
       
True

       
False

4.
True or False? Falling objects that land in machinery or on energized equipment may 


create secondary hazards.
       
True

       
False

5.
True or False? An open-sided platform next to dangerous equipment does not require 

a railing if the platform is less than four feet off the ground. 

       
True

       
False

6.
True or False? “Cages” and “wells” are no longer considered adequate fall protection for 


fixed ladders.
      
True

       
False

7.
True or False? Handrails for stairs must have at least 3 inches of clearance around them, 


so you can get a good grip on them. 

       
True

       
False

8.
True or False? To help people keep their balance and avoid falling, all stairways with four or more steps must have railings.
       
True

       
False

9.
True or False? It is safe to use a portable ladder horizontally as a scaffold or work platform.
       
True

       
False

10.
True or False? Scaffolds with work platforms 10 feet or more off the ground are required to have their open sides protected by railings with mid-rails and toeboards.
       
True

       
False
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