QUIZ
"WALKING AND WORKING SURFACES IN 

CONSTRUCTION ENVIRONMENTS"
PRESENTER'S COPY... WITH ANSWERS 
1.
True or False? Construction work can require you to work in rough or unfinished work environments.
   X   
True

       
False

2.
True or False? Anything that comes between the soles of your boots and the ground 


can cause you to slip.
   X   
True

       
False

3.
True or False? Barriers must be installed on all open-sided platforms and catwalks that 


are four feet or more off the ground, to help prevent falls.
   X   
True

       
False
4.
True or False?  Falling objects that land in machinery or on energized equipment may 

create secondary hazards.
   X   
True

       
False

5.
True or False? An open-sided platform next to dangerous equipment does not require a 

railing if the platform is less than four feet off the ground.
      
True

    X   
False

6.
True or False? “Cages” and “wells” are no longer considered adequate fall protection for 

fixed ladders.
   X   
True

       
False

7.
True or False? Handrails for stairs must have at least 3 inches of clearance around them, 

so you can get a good grip on them.
   X   
True

       
False

8.
True or False? To help people keep their balance and avoid falling, all stairways with four or more steps must have railings.
   X   
True

       
False

9.
True or False? It is safe to use a portable ladder horizontally as a scaffold or work platform.
      
True

    X   
False

10.
True or False? Scaffolds with work platforms 10 feet or more off the ground are required to have their open sides protected by railings with mid-rails and toeboards.
   X   
True

       
False
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