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CONSTRUCTION ENVIRONMENTS"
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1.
True or False?  Construction work can require you to work in rough or unfinished work environments.
       
True

       
False

2.
True or False? Anything that comes between the soles of your boots and the ground 


can cause you to slip.
       
True

       
False

3.
True or False? Barriers must be installed on all open-sided platforms and catwalks that 


are four feet or more off the ground, to help prevent falls.
       
True

       
False
4.
True or False? Falling objects that land in machinery or on energized equipment may 


create secondary hazards.
       
True

       
False

5.
True or False? An open-sided platform next to dangerous equipment does not require 

a railing if the platform is less than four feet off the ground. 

       
True

       
False

6.
True or False? “Cages” and “wells” are no longer considered adequate fall protection for 


fixed ladders.
      
True

       
False

7.
True or False? Handrails for stairs must have at least 3 inches of clearance around them, 


so you can get a good grip on them. 

       
True

       
False

8.
True or False? To help people keep their balance and avoid falling, all stairways with four or more steps must have railings.
       
True

       
False

9.
True or False? It is safe to use a portable ladder horizontally as a scaffold or work platform.
       
True

       
False

10.
True or False? Scaffolds with work platforms 10 feet or more off the ground are required to have their open sides protected by railings with mid-rails and toeboards.
       
True

       
False
CST-494
