QUIZ
"WALKING AND WORKING SURFACES IN HEALTHCARE ENVIRONMENTS… FOR OFFICE AND FACILITIES PERSONNEL"
PRESENTER'S COPY... WITH ANSWERS 
1.
True or False? The weight-bearing capacity of a floor can normally be determined by 


a visual inspection of its surface.
      
True

    X   
False

2.
True or False? Good housekeeping practices can prevent many slips, trips and falls.
   X   
True

       
False

3.
True or False? It is safe to use a portable ladder horizontally as a scaffold or work platform.
      
True

    X   
False

4.
True or False?  Falling objects that land in machinery or on energized equipment may 


create secondary hazards.
   X   
True

       
False

5.
True or False? Openings in floors pose more of a threat than openings in walls do.
      
True

    X   
False

6.
True or False? “Cages” and “wells” are no longer considered adequate fall protection for 


fixed ladders.
   X   
True

       
False

7.
True or False? Handrails for stairs must have at least 3 inches of clearance around them, 


so you can get a good grip on them.
   X   
True

       
False

8.
True or False? To help people keep their balance and avoid falling, all stairways with four or more steps must have railings.
   X   
True

       
False

9.
True or False? It is safe to use a portable ladder horizontally as a scaffold or work platform.
      
True

    X   
False

10.
True or False? Scaffolds with work platforms 10 feet or more off the ground are required to have their open sides protected by railings with mid-rails and toeboards.
   X   
True

       
False
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