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Insane Synergy Cracker Box Set Up Sheet

1) Engine Placement – 18 5/16 inches from the back of the transom to the center of the spark plug.

2) Skag Placement – 18” inches from the back of the skag to the back of the transom.  The skag is a shark tooth design.

3) Strut Placement – Center of the back of the transom.

4) Hardware Placement – Center of transom
5) Turn Fin Placement – Mount the turn fin at 90 degrees from the bottom of the hull out flush on the right side of the hull.  The turn fin should hang 1 ½ inches below the hull.

6) Cavitation Plates Placement – The left cavitation plate should be placed 3/16th’s of an inch off the side of the hull and flush with the bottom of the hull.  The right cavitation plate should have a ¼” gap between the cavitation plate and the turn fin.  This should also be mounted flush with the bottom of the hull.

7) Gas Tank Placement – The gas tank should be mounted directly across from the motor on the right side of the hull and up against the side of the hull.

Tips:

Before your first run, here are some adjustment suggestions:

· Set the strut 9/16” from the bottom of the hull to the center of the prop shaft.  This will be a good starting point. {approximately 3 degrees negative on the strut}

· Adjust the left cavitation plate down 1/8th of an inch. 

· Adjust the right cavitation plate flush with the bottom of the hull.

Prop Recommendations for subsurface:

· Prop Works West  6514 – 330
· Prop Works West  6517 – 355 or 365
