Lumen-King Gold Series 720W LED

The Gold Series 720W is Lumen King's high-efficiency LED grow light: 3.15 µmol/J efficacy and a PPF of 2268 µmol/s from just 720W of input power. For growers who want the maximum output per watt, this is the fixture to beat.

Its full-spectrum output supports both the vegetative and flowering phases, replicating natural sunlight for robust plant health from seedling to harvest. The dimmable driver (0-10V signal or knob) lets you fine-tune intensity, while the Lumen King Eco Controller (sold separately) allows centralized management of up to 30 fixtures — ideal for large-scale operations.

Like every Lumen King fixture, the Gold Series 720W uses a foldable six-bar design for quick installation and storage, distributes light uniformly across the canopy to eliminate hotspots, and runs silently on passive cooling with no fans to fail.

Built to professional standards: full-spectrum output, CE/UKCA/RoHS certification, an IP44 rating and a 2-year warranty.
