**FITTING INSTRUCTIONS HANDWOVEN AND SISAL CARPETS ITC INTERNATIONAL LUXURY FLOORING.**

* **HANDWOVEN CARPET IS LABOR INTENSIVE .**
* **MEASURE CAREFULLY .**
* **INSPECT CARPET ON FAULTS BEFORE INSTALLATION.**
* **3 % TOLERANCE IS RECOMMENDED IN ORDERRING.**
* **IN CASE OF GRIPPERS TAKE 0.5 - 1 CM SPACE TO THE SKIRTING.**
* **IN CASE OF SEAMING: USE SEAMING TAPE**
* **CARPET SHOULD BE INSTALLED BY PROFESSIONALS.**
* **IN CASE OF SEAMING FOR HANDWOVEN: ALWAYS TO BE CUT IT FROM THE BACKSIDE OF THE CARPET.**
* **CARPET MAY STRECTCH ONTO DOUBLE GRIPPERS OVER GOOD QUALITY SOLID UNDERLAY.**
* **CARPET MAY ALSO BE STUCK DIRECTLY ON FLOOR.**
* **CARPET CAN BE FITTED OVER UNDERLAY USING THE DOUBLE STICK METHOD.**
* **THE BLACK OR WHITE CLOTH ON EACH BACKING IS AS PROTECTION AND IT MIGHT HAPPEN THAT COTTON CLOTH COME LOOSE.**
* **IT THIS OCCURS YOU HAVE TWO OPTIONS;**
* **YOU REMOVE THE COTTON CLOTH ( THIS IS EASY ) AND YOU INSTALL CARPET ON THE ORGINAL BACKING OR**
* **YOU GLUE COTTON CLOTH ON BACKING AND THEN INSTALL THE CARPET.**
* **OUR RECOMMENDATION IS TO INSTALL CARPET ON COTTON CLOTH.**
* **WHAT METHOD YOU USE : IT WILL NOT AFFECT THE BEAUTY OF THE CARPET.**
* **HANDFITTING VIDEO ON YOU TUBE**

**PLEASE NOTE:**

**IN SOME HANDWOVEN CUT AND LOOP CARPETS THE LINES MAY RUN OUT ALONG THE SEAMS.**

**FOR THIS REASON, THE POSITIONS OF ANY SEAMS SHOULD BE PLANNED WITH CARE.**

**HAND WOVEN CARPETS ARE FINISHED BY HAND , SO PILE HEIGHTS CAN VARY SLIGHTLY AND A LIGHT SHEAR MAY OCCASIONALLY BE NECESSARY ALONG THE SEAMS.**

**FITTING INSTRUCTIONS SISAL.**

* **BEFORE YOU INSTALL SISAL, PLEASE NOTE THE FOLLOWING:**
* **AS SISAL CAN SHRINK YOU NEED TO TAKE EXTRA M 1 FROM 10 % WITH A MINUMUM OF 10 CM TO CORRECT ANY DEVIATIONS.**
* **TEMPATURE IN ROOM NEED TO BE MINIMAL 14 % .**
* **THE CARPET NEED TO ACLLIMATISE 24 HOURS IN SPACE WHERE CARPET WILL BE INSTALLED.**
* **PLEASE INSPECT CARPET ON FAULTS BEFORE INSTALLATION .**
* **THE SUBFLOOR NEED TO BE DRY, FIRM AND LEVEL.**
* **LAY STRIPS OF CARPET NEXT TO EACHOTHER WITH AN OVERLAP IN ORDER TO ABSORB STRETCH AND SHRINKING .**
* **THE FIRST STRIP ALWAYS ALONG THE SIDE OF THE ROOM.**
* **WE RECOMMEND TO GLUE THE CARPET.**
* **CUT THE STIPS ALONG THE WARP.**
* **USE A KNEE STRECTHER TO PLACE SEAMS FROM THE STRIPS TIGHTLY AGAINST EACHOTHER.**
* **SISAL NEED TO BE GLUED WITH CARE AGAINST THE SKIRTING TO PREVENT FRAYING.**
* **YOU ALWAYS CAN USE CUT – RESISTANT SPRAY.**
* **SEAMS COULD BE VISIBLE.**