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Section 1: Identification of the substance/mixture and of the company/undertaking
1.1 Product identifier
Trade name: STARCOAT PMMA MORTAR
1.2 Relevant identified uses of the substance or mixture and uses advised against See Section 16
Application of the substance / the mixture Binder
1.3 Details of the supplier of the safety data sheet
Supplier	Address
Tel: 
Email: 

1.4 Emergency telephone	Company name and emergency telephone number
In the event of a medical enquiry involving this product, members of the public should contact:
NHS 111
a doctor or
a local hospital accident and emergency department.

The NPIS (National Poisons Information Service) helpline is available for enquiries from medical professionals only.
Tel: 0344 892 0111



Section 2: Hazards identification
2.1 Classification of the substance or mixture
[image: ]Classification according to Regulation (EC) No 1272/2008


GHS02 flame


[image: ]Flam. Liq. 3	H226 Flammable liquid and vapour.


GHS07


Skin Irrit.2	H315 Causes skin irritation
Eye Irrit.2	H319 Causes serious eye irritation
Skin Sens.1	H317 May cause an allergic skin reaction
STOT SE 3	H335 May cause respiratory irritation
2.2 Label elements
Labelling according to Regulation (EC) No 1272/2008
The product is classified and labelled according to the CLP regulation.
[image: ]Hazard pictograms
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Signal word Warning
Hazard determining components of labelling:
Methyl methacrylate Benzyl methacrylate 2-ethylhexyl acrylate
Hazard statements
H226	Flammable liquid and vapour
H315	Causes skin irritation
H319	Causes serious eye irritation
H317	May cause an allergic skin reaction
H335	May cause respiratory irritation
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Precautionary statements
P210	Keep away from heat, hot surfaces, sparks, open flames and other ignition surfaces. - No smoking.
P261	Avoid breathing in fumes.
P280	Wear protective gloves/ eye protection.
P303+P361+P353	IF ON SKIN (or HAIR): Remove all contaminated clothing immediately. Rinse skin with water/shower.
P312	Call a POISON CENTRE/ doctor if you feel unwell.
P403+P233	Store in a well-ventilated place. Keep container tightly closed.
2.3 Other hazards
Results of PBT and vPvB assessment
PBT: Does not meet the PBT-criteria of Annex XIII of REACH (self assessment).
vPvB: Does not meet the vPvB-criteria of Annex XIII of REACH (self assessment).


Section 3: Composition/information on ingredients
3.2	Mixtures
Description: Mixture of substances listed below with nonhazardous additions.

	Dangerous components:

	CAS: 80-62-6
	methyl methacrylate
	25-50%

	EINECS: 201-297-1
	Flam. Liq. 2, H225; Skin Irrit.2, H315; Skin Sens.1, H317; STOT SE 3, H335
	

	Reg No.
	
	

	01-2119452498-28-0000
	
	

	01-2119452498-28-0025
	
	

	01-2119452498-28-0028
	
	

	CAS: 2495-37-6
	Benzyl methacrylate
	25-50%

	EINECS: 219-674-4
	Skin Irrit.2, H315; Eye Irrit.2, H319, Skin Sens.1, H317; STOT SE 3, H335
	

	Reg No. 01-2119960155-39-0000
	
	

	CAS: 103-11-7
	2-ethylhexyl acrylate
	>10->20%

	EINECS: 203-080-7
	Skin Irrit.2, H315; Skin Sens.1, H317; STOT SE 3, H335,
	

	Reg No. 01-2119453158-37
	Aquatic Chronic 3, H412
	


Additional information: For the wording of the listed risk phrases refer to section 16.


Section 4: First aid measures
4.1 Description of first aid measures General information:
Immediately remove any clothing soiled by the product. Take affected persons out of danger area and lay them down. Involve a doctor immediately.
After inhalation:
In case of unconsciousness place patient stably in side position for transportation. Take affected persons into fresh air and keep them quiet.
Seek medical treatment.
After skin contact:
Immediately wash with water and soap and rinse thoroughly. If skin irritation continues, consult a doctor.
After eye contact: Rinse opened eye for several minutes under running water. Then consult a doctor.
After swallowing: Do not induce vomiting; call for medical help immediately.
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4.2 Most important symptoms and effects, both acute and delayed
Headache Dizziness
Skin sensitization
Irritant to skin, eyes and respiratory system
4.3 Indication of any immediate medical attention and special treatment needed
After inhalation, even in the absence of signs of illness, give inhaled Corticoid (e.g. Ventolair).


Section 5: Firefighting measures
5.1 Extinguishing media
Suitable extinguishing agents: CO2, sand, extinguishing powder, foam.
For safety reasons unsuitable extinguishing agents: Water with full jet
5.2 Special hazards arising from the substance or mixture
Can form explosive gas-air mixtures.
Formation of toxic gases is possible during heating or in case of fire. In case of fire, the following can be released:
Carbon monoxide (CO) Nitrogen oxides (NOx)
Vapours are heavier than air. Crawling vapours can travel some distance from the source of ignition.
5.3 Advice for firefighters Protective equipment:
Wear fully protective suit.
Wear self-contained respiratory protective device.
Additional information
Cool endangered receptacles with water spray.
Collect contaminated fire fighting water separately. It must not enter the sewage system.


Section 6: Accidental release measures
6.1 Personal precautions, protective equipment and emergency procedures
Ensure adequate ventilation Keep away from ignition sources.
Use respiratory protective device against the effects of fumes/dust/aerosol. Wear protective equipment. Keep unprotected persons away.
6.2 Environmental precautions:
Do not allow to enter sewers/ surface or ground water.
Inform respective authorities in case of seepage into water course or sewage system.
6.3 Methods and material for containment and cleaning up:
Do not flush with water or aqueous cleansing agents
Absorb with liquid-binding material (sand, diatomite, acid binders, universal binders, sawdust).
6.4 Reference to other sections
See Section 7 for information on safe handling.
See Section 8 for information on personal protection equipment. See Section 13 for disposal information.
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Section 7: Handling and storage
7.1 Precautions for safe handling
Cool down container if it heats up. Containers exposed to heat should be cooled with water. Near heat, keep containers of water available. Emergency cooling must be available in the case of a fire nearby.
Keep containers closed to protect against heat build up (pressure rise). Avoid heat. Do not refill residue into storage receptacles.
Ensure good ventilation/exhaustion at the workplace, (at least 7 air changes), especially at floor level. (Fumes are heavier than air).
Prevent formation of aerosols.
Information about fire - and explosion protection:
Highly volatile, flammable constituents are released during processing. Keep ignition sources away - Do not smoke.
Fumes can combine with air to form an explosive mixture. Only explosion-proof equipment.
Protect against electrostatic charges. Protect from heat.
7.2 Conditions for safe storage, including any incompatibilities Storage:
Requirements to be met by storerooms and receptacles:
Store only in the original receptacle. Store in a cool location.
Information about storage in one common storage facility:
Store away from oxidising agents. Store away from foodstuffs.
Further information about storage conditions:
Store in cool, dry conditions in well sealed receptacles. Storage in a collecting room is required.
Store under lock and key and with access restricted to technical experts or their assistants only. Max storage temperature 30°C.
Keep container tightly sealed. Protect from heat and direct sunlight.
7.3 Specific end use(s) Building coating or sealing.
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Section 8: Exposure controls/personal protection
Additional information about design of technical facilities: No further data; see item 7.
8.1 Control parameters

	· Ingredients with limit values that require monitoring at the workplace:

	80-62-6- methyl methacrylate (25-50%)

	WEL
	Short-term value: 416 mg/m³, 100 ppm
Long-term value: 208 mg/m³, 50 ppm

	DNELs

	80-62-6 methyl methacrylate

	Inhalative
	DNEL (worker)



DNEL (population)
	210 mg/m³ (Long-term - local effects) 210 mg/m³ (Long-term – systemic effects) Long-term

74.3 mg/kg (Long-term - systemic effects) 105 mg/m³ (Long-term - local effects)

	2495-37-6 benzyl methacrylate

	Dermal Inhalative
	DNEL (worker) DNEL (worker)
	6.94 mg/cm3 (Long-term – systemic effects)
24.2 mg/cm3 (Long-term – systemic effects)

	103-11-7 2-ethylhexyl acrylate

	Dermal

Inhalative
	DNEL

DNEL
	242 μg/cm3 (Employee / Industrial / Commercial) Long term and short term
37.5 mg/kg (Employee / Industrial / Commercial) (long term)

	PNECs

	80-62-6 methyl methacrylate

	PNEC
(sediment) PNEC
	1.47 mg/kg dw (ground)
5.74 mg/kg dw (freshwater)
0.094 mg/l (seawater)
0.94 mg/l (freshwater)

	2495-37-6 benzyl methacrylate

	PNEC
	0.00216 mg/l (seawater)

	103-11-7 2-ethylhexyl acrylate

	Ground

PNEC
Water
	2.3 mg/l (Soil microorganisms) 1 mg/l (ground)
0.0023 mg/kg (oral intake)
0.126 mg/l (sediment) 0.002727 mg/l (fresh water)


Additional information: The lists valid during the making were used as a basis.
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8.2 Exposure controls
Personal protective equipment:
[image: ][image: ][image: ]
General protective and
hygienic measures	Avoid contact with the eyes and skin.
Immediately remove all soiled and contaminated clothing. Wash hands before breaks and at the end of work.
Keep away from foodstuffs, beverages and food. Do not inhale gases / fumes / aerosols.·
Respiratory protection	Ensure good ventilation.
Inside buildings and when limits are exceeded, use respiratory filter device: Filter type A1; at higher concentrations and prolonged exposure use air recycling independent breathing apparatus
type A2.
Protection of hands	Protective gloves
Glove material has to be impermeable and resistant to the product/ the substance/ the preparation. Select glove material on consideration of the penetration times, rates of diffusion
and degradation.
Preventive skin protection by use of skin-protecting agents is recommended. After use of gloves apply skin-cleaning agents and skin cosmetics.
Check protective gloves prior to each use for their proper condition. Due to missing tests no recommendation to the glove material can be given for the product/ the preparation/ the chemical mixture.
Material of gloves	The selection of suitable gloves does not only depend on the material, but also on further marks of quality and varies
from manufacturer to manufacturer. As the product is a preparation of several substances the resistance of the glove material cannot be calculated in advance and has therefore to be checked prior
to the application.
Protective gloves according to EN 374. Suitable material: nitrile.
Penetration time of glove material  Our recommendation is mainly for a once-only use as a short-term
protection against liquid splashes. For other applications, you should contact a glove manufacturer.
The exact break through time must be found out from the manufacturer of the protective gloves and must be observed.
For permanent contact in work areas without heightened risk
of injury (e.g. Laboratory), gloves made of the following material
are suitable	Butyl rubber, BR
For permanent contact, gloves made of the following materials
are suitable	Butyl rubber, BR
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Not suitable are gloves made
of the following material	Leather
Eye protection	Tightly sealed goggles, EN-Standard: EN 166
Body protection	Protective work clothing


Section 9: Physical and chemical properties
9.1 Information on basic physical and chemical properties General Information
Appearance:
Form:	Fluid
Colour:	Unpigmented
Odour:	Ester-like
Odour threshold:	Not determined
pH-value:	Not determined
Change in condition
Melting point/Melting range:	Undetermined
Boiling point/Boiling range:	101 °C (MMA)
Flash point:	23 °C (EN ISO 3680)
Flammability (solid, gas):	Not applicable
Ignition temperature:	252°C (2-EHA)
Decomposition temperature:	Not determined
Self-igniting temperature:	Product is not self-igniting.
Danger of explosion:	Product is not explosive. However, formation of explosive air/ vapour
mixtures is possible.
Explosion limits:
Lower:	1.65 Vol %(MMA)
Upper:	12.5 Vol % (MMA)
Vapour pressure at 20 °C	38.7hPa (MMA)
Density at 20 °C:	1 g/cm³ (EN ISO 2811-1)
Relative density	Not determined
Vapour density	Not determined
Evaporation rate	Not determined
Solubility in / Miscibility with water: Not miscible or difficult to mix.
Partition coefficient
(n-octanol/water):	log Pow: 4.29 (2-EHA); (25°C, OECD 107) log Pow: 1.38 (MMA)
Viscosity:
Dynamic	Not determined.
Kinematic at 20 °C	25s (ISO 6mm)
Solvent content:
VOC (EC)	0.00%
Solids content:	33.1%
9.2 Other information	No further relevant information available.
Ref: XXXX
Version   Date

07
STARCOAT PMMA MORTAR
LIQUID WATERPROOFING




Section 10: Stability and reactivity
10.1 Reactivity see Section 10.2
10.2 Chemical stability
Thermal decomposition / conditions to be avoided:
No decomposition if used according to specifications.
10.3 Possibility of hazardous reactions
Exothermic reaction.
Reacts with peroxides and other radical forming substances.
A hazardous polymerization may occur after the exhaustion of the inhibitor.
10.4 Conditions to avoid: Heat and direct sunlight.
10.5 Incompatible materials: Reacts with peroxides and other free-radical generators.
10.6 Hazardous decomposition products:
No dangerous decomposition when product used according to specifications.
Additional information:
Emergency procedures will vary depending on individual circumstances. The customer should have a contingency plan at the workplace where the product is present.

Section 11: Toxicological information
11.1 Information on toxicological effects There were no toxicological findings to the mixture.
Acute toxicity Based on available data, the classification criteria are not met.

	LD/LC50 values relevant for classification:

	80-62-6 methyl methacrylate

	Oral



Dermal Inhalative
	LD50 NOAEL


LC50 NOAEL


LC50/4h
	>5000 mg/kg (rat) (OECD 401)
2000 ppm (rat)
Drinking water, 6-2000 ppm Findings: no toxic effects
>5000 mg/kg (rabbit)
25 ppm (rat)
24 – 400 ppm
Findings: damage to mucous membranes in the nose at 400 ppm
29.8 mg/l (rat)

	2495-37-6 benzyl methacrylate

	Oral Dermal
	LD50 LD50
	3980 mg/kg (rat) (OECD 401)
>2000 mg/kg (rat) (Acute dermal toxicity)

	103-11-7 2-ethylhexyl acrylate xide

	Oral Dermal
	LD50 LC50
	4435 mg/kg (rat) (BASF Test) 7520 mg/kg (hare)


Primary irritant effect:
Skin corrosion/irritation	Causes skin irritation and irritability.
Serious eye damage/irritation	Causes serious eye irritation. Respiratory or skin sensitization	May cause an allergic skin reaction. Other information (about experimental toxicology):
Due to the high vapour pressure a harmful concentration in the air is quickly reached. At high concentrations a narcotic effect can occur.
Subacute to chronic toxicity:	Not tested.
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Toxiokinetics, metabolism
and distribution	The drug is metabolized rapidly (MMA).
Repeated dose toxicity	No data available.
CMR effects (carcinogenicity, mutagenicity and toxicity
for reproduction)	Not tested.
Germ cell mutagenicity	Based on available data, the classification criteria are not met. Carcinogenicity	Based on available data, the classification criteria are not met. Reproductive toxicity	Based on available data, the classification criteria are not met. STOT-single exposure	May cause respiratory irritation.
STOT-repeated exposure	Based on available data, the classification criteria are not met.
Aspiration hazard	Based on available data, the classification criteria are not met.


Section 12: Ecological information
12.1 Toxicity

	80-62-6 methyl methacrylate

	EC3/16h
	100 mg/l (Pseudomonas putida) (Cell proliferation inhibition test Bringmann-Kuehn)

	2495-37-6 benzyl methacrylate

	EC10/21d
	3.34mg/l (daphnia magna) (OECD 211)

	Aquatic toxicity

	80-62-6 methyl methacrylate

	EC50/48h LC50/96h EC50/72h NOEC/72h EC50/72h NOEC
	69 mg/l (daphnia magna) (OECD 202)
>79 mg/l (Rainbow trout) (OECD 203)
>110 mg/l (Pseudokirchneriella subcapitata) (OECD 201)
>110 mg/l (Selenastrum capricornutum) (OECD 201)
>110 mg/l (Selenastrum capricornutum) (OECD 201)
9.4 mg/l (Danio rerio) (OECD 210) Fish early life stage test, 35 days
37 mg/l (daphnia magna) (OECD 211)
21 days

	2495-37-6 benzyl methacrylate

	LC50/48h EC50/72h
	4.67 mg/l (fish)
2.28mg/l (Desmodesmus subspicatus) (OECD 201)

	103-11-7 2-ethylhexyl acrylate

	Other (28d)


EC50/48h (static) LC50/96h (static) NOEC/21d
	>1000 mg/kg (Soil microorganisms) (OECD 217)
The product has not been tested. The statement has been derived from products of a similar structure or composition.
1.3 mg/l (daphnia magna) (OECD 202, Part 1)
1.81 mg/l (Rainbow trout) (OECD 203)
0.19 mg/l (daphnia magna)
The details of the toxic effect relates to the analytically determined concentration. The product has not been tested. The statement has been derived from products of a similar structure or composition.

	EC50/72h (static)
	1.71 mg/l (scenedesmus subspicatus) (OECD 201)
The details of the toxic effect relates to the analytically determined concentration.
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12.2 Persistence and degradability No further information available. Other information: The product is easily biodegradable.
12.3 Bioaccumulative potential
2-EHA: can be accumulated in organisms; biocaccumulation potential: Bioconcentration Factor 282.4 (Calculated).
12.4 Mobility in soil
MMA: A binding to the solid phase of soil, sediment and sewage sludge is not expected. From the water surface the substance is slowly evaporated into the atmosphere. 2-EHALL: the product floats on water and does not dissolve. Absorption in soil is not likely.
Additional ecological information:
COD-value: 2-EHA: Theoretical oxygen demand (TOD) = 5.6 g / g
BOD5-alue: 0.14 g/g (MMA)
General notes:
Water hazard class 1 (German Regulation) (Self-assessment): slightly hazardous for water Do not allow product to reach ground water, water course or sewage system..
12.5 Results of PBT and vPvB assessment
PBT: Does not meet the PBT-criteria of Annex XIII of REACH (self assessment).
vPvB: Does not meet the vPvB-criteria of Annex XIII of REACH (self assessment).
12.6 Other adverse effects No further relevant information available.


Section 13: Disposal considerations
13.1 Waste treatment methods
Hazardous waste according to Waste Catalogue (EWC). If recycling is not possible, waste must be removed in compliance with local regulations.
Recommendation
[image: ]Uncured product residues are special waste. Cured product residues are not hazardous waste.


Must not be disposed together with household rubbish. Do not allow product to reach sewage system.

Waste disposal key:
The following Waste Codes of the European Waste Catalogue (EWC), are considered a recommendation. The disposal must be coordinated with the local waste disposal company.
Liquid product:
080409* adhesive and sealants containing organic solvents or other dangerous substances 080410 adhesives and sealants containing wastes other than those mentioned in 080409
Cured product:
170 203 plastic
Uncleaned packaging:
Recommendation:
This material and its container must be disposed of as hazardous waste. Disposal must be made according to official regulations.
[image: ]
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Section 14: Transport information
14.1 UN-Number	Void
ADR, IMDG, IATA	UN1263
14.2 UN proper shipping name
ADR	1263 PAINT
IMDG IATA	PAINT
14.3 Transport hazard class(es) ADR, IMDG, IATA
[image: ]
Class	3 Flammable liquids.
Label	3
14.4 Packing group
ADR, IMDG, IATA	IIII
14.5 Environmental hazards:
Marine pollutant:	No
14.6 Special precautions for user	Warning: Flammable liquids
Danger code (Kemler)	30
EMS Number:	F-E,S-E
Stowage Category	A
14.7 Transport in bulk according to Annex II of MARPOL and the IBC Code	Not applicable.
Transport/Additional information:
ADR
Limited Quantities (LQ)	5L
Excepted Quantities (EQ)	Code: E1
Maximum net quantity per inner packaging: 30ml Maximum net quantity per inner packaging:1000ml
Transport category	3
Tunnel restriction code	D/E
IMDG
Limited Quantities (LQ)
Excepted Quantities (EQ)	5L
UN “Model Regulation”	Code: E1
Maximum net quantity per inner packaging: 30ml Maximum net quantity per inner packaging:1000ml
UN “Model Regulation”	UN 1263 PAINT, 3, III



Section 15: Regulatory information
15.1 Safety, health and environmental regulations/legislation specific for the substance or mixture Directive 2012/18/EU
Named dangerous substances - ANNEX I None of the ingredients is listed.
Seveso category P5c FLAMMABLE LIQUIDS
Qualifying quantity (tonnes) for the application of lower-tier requirements 5,000 t Qualifying quantity (tonnes) for the application of lower-tier requirements 50,000 t REGULATION (EC) No 1907/2006 ANNEX XVII Conditions of restriction: 3
National regulations:
Information about limitation of use:
Employment restrictions under the Maternity Protection Directive (94/33/EC).
Employment restrictions for maternity Directive (92/85/EEC) for expectant and nursing mothers.
15.2 Chemical safety assessment: A Chemical Safety Assessment has not been carried out.


Section 16: Other information
These figures relate to the product as delivered.
Sector of Use
Relevant identified uses of the mixture
SU3 Industrial uses: Uses of substances as such or in preparations at industrial sites SU19 Building and construction work
SU22 Professional uses: Public domain (administration, education, entertainment, services, craftsmen)
Uses advised against
SU21 Consumer uses: Private households / general public / consumers
This information is based on our present knowledge. However, this shall not constitute a guarantee for any specific product features and shall not establish a legally valid contractual relationship.
Relevant phrases
H225	Highly flammable liquid and vapour
H315	Causes skin irritation
H317	May cause an allergic skin reaction
H319	Causes serious eye irritation
H335	May cause respiratory irritation
H412	Harmful to aquatic life with long lasting effects
Training hints
Training on hazards and precautions must be given prior to use and should be repeated at least annually thereafter.



Abbreviations and acronyms:
RID: Règlement international concernant le transport des marchandises dangereuses par chemin de fer (Regulations Concerning the International Transport of Dangerous Goods by Rail)
ICAO: International Civil Aviation Organisation
ADR: Accord européen sur le transport des marchandises dangereuses par Route (European Agreement concerning the International Carriage of Dangerous Goods by Road) IMDG: International Maritime Code for Dangerous Goods
IATA: International Air Transport Association
GHS: Globally Harmonised System of Classification and Labelling of Chemicals EINECS: European Inventory of Existing Commercial Chemical Substances ELINCS: European List of Notified Chemical Substances
CAS: Chemical Abstracts Service (division of the American Chemical Society)
VOC: Volatile Organic Compounds (USA, EU) DNEL: Derived No-Effect Level (REACH) DNEL: Derived No-effect level (REACH)
PNEC: Predicted No-Effect Concentration (REACH) LC50: Lethal concentration, 50 percent LC50: Lethal concentration, 50 percent
LD50: Lethal dose, 50 percent
PBT: Persistent, Bioaccumulative and Toxic vPvB: very Persistent and very Bioaccumulative
Flam. Liq. 2: Flammable liquids, Hazard Category 2 Flam. Liq. 3: Flammable liquids, Hazard Category 3 Skin Irrit. 2: Skin corrosion/irritation – Category 2
Eye Irrit. 2: Serious eye damage/eye irritation – Category 2 Skins Sens 1: Skin sensitization – Category 1
STOT SE 3: Specific target organ toxicity - Single exposure, Category 3
Aquatic Chronic 3: Hazardous to the aquatic environment – long-term aquatic hazard – Category 3
Sources:
www.gestis.de www.echa.eu logkow.cisti.nrc.ca



The information provided in this document is accurate to the best of our knowledge. The document does not constitute a specification and Axter takes no responsibility for the suitability of the product in a particular use. It is the user’s responsibility to ensure that the product is suitable for the intended application and use and to take
the necessary precautions to ensure that during handling, storage and installation of the product, all regulations to guarantee safety of people and the environment are observed. For further information or technical design assistance, contact Axter Ltd.

The data contained in this SDS has been supplied as required by the EC REACH Regulation No. 1907/2006 and the EC Regulation No. 1272/2008 on classification, labelling and packaging of substances and mixtures (CLP) for the purpose of protecting the health and safety of industrial and commercial users who are deemed capable of
understanding and acting on the information provided. Please ensure that it is passed to the appropriate person(s) in your company who are capable of acting on the information.

Disclaimer:
XXXX reserves the right to modify and update this data at any time without prior notice. Only the latest version of this document is valid, available for download at XXXX. Once downloaded, documents are uncontrolled. Users should always confirm they are referring to the latest version prior to use. Further assistance is available from XXXX,
Email: XXXX telephone: XXXX

The intended use of this product should be verified with XXXX prior to adoption to ensure its suitability and compliance with specifications, project requirements, industry regulations, legislation, good practice, installation techniques and all other relevant guidance. The user should ensure all necessary precautions are taken during handling, storage, installation and disposal of the product, and all regulations to guarantee safety of people and the environment are observed. XXXX accepts no liability for non-compliant use of this product.
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