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STK WESTERN RED CEDAR – 711R1 T&G
Where natural wood beauty and high fire resistance are required
[image: Mataverde SaferWood 1x6 STK Western Red Cedar siding, 711 T&G profile]
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Size: 1x6 nominal, 11/16" thick x 5" width (coverage)
Profile: Tongue and Groove (T&G), 711R profile w/resawn face
[image: 711R profile is a reversible siding option, v-grooved on both sides with a smooth and resawn face]
Treatment: Thermex-FR, FIRE RETARDANT TREATED WOOD
· WUI and IWUIC Compliant			• Class A (E-84 Extended 20-Minute)
· Non-Toxic Materials				• Paintable Stainable
· Limited Lifetime Warranty			• Indoor / Outdoor use
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Fire-Retardant Treated Wood
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