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PLANTERLITE — PRODUCT RANGE
	Range
	Shape
	Size range (mm)
	Weight (kg)
	Colourways / finish

	Rustic Bowls
	Bowl
	Ø280–1100 × H210–720
	2.5–50
	Rustic, Dark Grey, Sand

	Rustic Bench
	Bench trough
	L1100 × D400 × H420
	25
	Rustic, Dark Grey, Sand

	Corten Troughs
	Trough
	L600–1200 × D280–600 × H280–600
	8.5–35
	Corten (weathering-steel finish)

	Corten Cylinders
	Cylinder
	Ø250–1000 × H250–1000
	4.0–60
	Corten (weathering-steel finish)

	Corten Boxes
	Box
	L240–500 × D240–500 × H240–500
	4.0–18
	Corten (weathering-steel finish)

	Chelsea Boxes
	Box
	L220–650 × D220–650 × H220–650
	3.0–25
	Chelsea (natural finish)

	Chelsea Troughs
	Trough
	L500–1000 × D160–450 × H170–450
	4.5–25
	Chelsea (natural finish)

	Chelsea Cylinders
	Cylinder
	Ø220–650 × H220–650
	3.0–25
	Chelsea (natural finish)

	Smooth Urban Troughs
	Trough
	L600–1000 × D280–450 × H280–450
	8.5–30
	Black, Grey, White

	Smooth Urban Boxes
	Box
	L240–500 × D240–500 × H240–500
	4.0–18
	Black, Grey, White

	Terracotta Lined Pot
	Lined pot
	Ø250–730 × H190–540
	3.0–35
	Terracotta

	Patterned Outdoor Planters
	Planter
	Ø250–500 × H250–500
	3.0–13
	Flower / Tropical / Geometric / Fern – Dark Grey & White Grey


171 SKU variants across 19 ranges and multiple colourways. Sizes and weights shown are min–max across each range — full SKU codes, barcodes and pricing available on request.

	TYPICAL SIZING (GENERAL GUIDE)
	Dimension
	Minimum
	Maximum

	Width (W)
	250 mm
	500 mm

	Height (H)
	250 mm
	500 mm


Indicative range for standard planters — individual lines vary, see Product Range table above.
	COMPOSITION & AVAILABILITY
Composition: magnesium & sand composite, pasted over a fibreglass mesh for added stability and frost resistance (>95% biodegradable content).
Available finishes: over 100 finishes and size variations available on request.




	ABOUT PLANTERLITE
Planterlite is an eco-friendly material that has demonstrated excellent resilience in many climates over the last decade.
Whilst it has similar qualities to Fibreclay, different manufacturing techniques and blends offer improved durability, UV resistance and colour stability (with no leaching).
Planterlite mostly consists of naturally occurring magnesium dredged from lakes and rivers. This is mixed with sand and coloured powder, before being pasted over a small fibreglass mesh for added stability and improved frost resistance.
Over 95% of the composite is biodegradable. The manufacture of Planterlite requires only a fraction of the energy used for other planter types, as it sets naturally without kiln firing or machine moulding.
KEY BENEFITS
Lightweight & roof-ready – up to 80% lighter than comparable concrete planters, ideal for rooftops, terraces and podiums.
Durable by design – magnesium-and-sand composite reinforced with a fibreglass mesh, giving excellent UV resistance, colour stability and frost resistance.
Low maintenance – easy to clean with no repainting, rust or corrosion.
Design flexibility – available in a wide range of contemporary shapes, sizes and colours.
Easy installation – lightweight construction simplifies handling, positioning and future relocation.
Built for commercial landscapes – suitable for residential, hospitality, commercial and public realm projects.
	CLIMATE TESTING
1. Climate Change Test (DIN EN 60068-2-38:2010): 240 hours. Samples remained structurally intact; minor surface pinholes observed after testing.
1. Artificial Weathering Test (DIN EN ISO 4892-3:2016): 500 hours. No visual surface change after artificial weathering.
MAINTENANCE & CARE
Planterlite planters are designed for durable, low-maintenance performance in both indoor and outdoor environments.
Cleaning
1. Clean regularly with warm water and a mild, pH-neutral detergent.
1. Use a soft cloth or non-abrasive brush for stubborn marks.
1. Rinse thoroughly and allow to dry.
1. Avoid abrasive cleaners, harsh chemicals and wire brushes.
Outdoor care
1. Keep drainage holes clear of soil and debris.
1. Remove standing water and organic build-up regularly.
1. Clean spills promptly to minimise staining.
1. Avoid metal tools and aggressive de-icing products during winter.
Indoor care
1. Dust and wipe surfaces regularly.
1. Where planting directly into the planter, use a suitable liner or drip tray and avoid overwatering.
Natural weathering: minor variations, surface imperfections and changes in colour or texture are natural characteristics and may develop over time.
Moving: empty planters before moving. Use suitable lifting equipment where required and avoid dragging across finished surfaces.
With routine cleaning and good drainage, Planterlite requires minimal ongoing maintenance.




PRODUCT RANGE GALLERY
Every Planterlite shape, grouped by range. Sizes shown are the full min–max span across each shape — see the Product Range table for individual SKUs.
Rustic
Planterlite's core range, spanning six shapes in three colourways: Rustic, Dark Grey and Sand.
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Bench trough
Rustic, Dark Grey and Sand finish — L1100 × W400 × H420mm, 25kg.
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Rustic Bowl planter
Rustic, Dark Grey or Sand finish — 280–1100 × H210–720mm, 2.5–50kg



OTHER RANGES
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Smooth Urban
Trough — L600–1000 × D280–450 × H280–450mm, 8.5–30kg
Box — L240–500 × D240–500 × H240–500mm, 4.0–18kg
Colours: Black, Grey, White
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Corten
Trough — L600–1200 × D280–600 × H280–600mm, 8.5–35kg
Cylinder — Ø250–1000 × H250–1000mm, 4.0–60kg
Box — L240–500 × D240–500 × H240–500mm, 4.0–18kg
Finish: weathering-steel Corten (single signature finish)
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Chelsea
Box — L220–650 × D220–650 × H220–650mm, 3.0–25kg
Trough — L500–1000 × D160–450 × H170–450mm, 4.5–25kg
Cylinder — Ø220–650 × H220–650mm, 3.0–25kg
Finish: Chelsea natural (single signature finish)
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Terracotta Lined Pot
Lined pot — 250–730mm × H190–540mm, 3.0–35kg
Finish: Terracotta (single signature finish)
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Patterned Outdoor Planters
Planter — Ø250–500 × H250–500mm, 3.0–13kg
Designs: Flower, Tropical, Geometric, Fern — in Dark Grey or White Grey
	



	▶ Find out more or request a sample
sales@kinleysystems.com
or visit kinleysystems.com
	© 2026 Kinley® Ltd. At the time of writing and publication of this sheet, all information is specified correctly. The company reserves the right to change the specifications of this product at any time without prior notice to third parties. Any images and diagrams used in this sheet are intended only as illustrations. No rights can be derived from them.
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