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Guidance notes to accompany Pre-Shipment Survey report (Goods)
1. Frozen / Chilled Cargo:
· For Frozen/chilled produce, please specify if integral or port hole reefer.  If port hole, was “clip on” unit fitted and working?
· Check set point temperature is correct and temperature of container prior to loading.  For chilled products, have goods been sufficiently pre-cooled prior to loading?
· Confirm mode of transport used to carry the consignment from shipper’s factory to port reefer container yard.
· Detail the date and time that loading commenced and was completed.

· Check temperature on container (on completion of loading).

· Check and report on ambient temperature. 

· Confirm the date the container was scheduled to be loaded onto the vessel and estimate date of arrival.
2. New / Used Machinery:
· For used machinery, state whether machine operational at the time of inspection or already dismantled.

· For both new and used, check the overall condition making specific reference to any areas which are rusted/scratched/broken/damaged.  Clear photographs should be taken of all areas.

· Record and photograph the date of manufacture and serial numbers of all parts, where present or available.

· If surveyor is instructed to witness the loading/securing operation, detail all methods used including types of handling/lifting and securing material.  In addition, also state whether the handling/loading/securing/stowage is considered to be appropriate.
· If machine to be road transported, provide details on length of anticipated travel, route conditions or any other pertinent information.
· Weather conditions (where/when relevant or appropriate).
· Mention and confirm in report any recommendation given to Carriers (Captain or truck driver) where considered valuable or important.


