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SPECIFICATION
Entrada Horizon Canopy NZ
Specification for the supply and installation of the Entrada Horizon aluminium canopy system with stainless steel tie rods. Written in NZ Masterspec format for inclusion in the project specification.
	Project
	[Project name]

	Specifier
	[Name and company]

	Date
	[DD/MM/YYYY]


1	GENERAL
This section relates to the supply and installation of the Entrada Horizon Canopy system. Entrada supplies the Horizon as a pre-finished, structurally calculated kitset, installed by an installer approved by Entrada.
1.1	ABBREVIATIONS AND DEFINITIONS
Refer to the general section 1232 INTERPRETATION & DEFINITIONS for abbreviations and definitions used throughout the specification.
DOCUMENTS
1.2	DOCUMENTS
Refer to the general section 1233 REFERENCED DOCUMENTS. The following documents are specifically referred to in this section:
	AS/NZS 1163
	Cold-formed structural steel hollow sections

	AS/NZS 1594
	Hot-rolled steel flat products

	AS/NZS 1664.1
	Aluminium structures - Limit state design

	AS/NZS 1734
	Aluminium and aluminium alloys - Flat sheets, coiled sheet and plate

	AS/NZS 1866
	Aluminium and aluminium alloys - Extruded rod, bar, solid and hollow shapes

	NZS 3404.1
	Steel structures Standard

	NZS 3404.2
	Commentary to the Steel structures Standard

	AS/NZS 3678
	Structural steel - Hot-rolled plates, floorplates and slabs

	AS/NZS 4600
	Cold-formed steel structures


1.3	MANUFACTURER/SUPPLIER DOCUMENTS
Manufacturer and supplier documents relating to this part of the work:
	Entrada
	Horizon Canopy Technical Data Sheet

	Entrada
	Care & Maintenance Manual (ENT-CM)



Manufacturer/supplier contact details
	Company
	Entrada (a division of Insol Ltd)

	Address
	7 Waokauri Place, Auckland

	Web
	entradacanopies.com

	Email
	enquiries@entradacanopies.com

	Telephone
	09 276 9735


1.4	SPECIFIC DESIGN DOCUMENTS
Specific design documents relating to this part of the work:
	Documents
	[List documents]

	Refer to
	[Drawing or document reference]


WARRANTIES
1.5	WARRANTY - MANUFACTURER/SUPPLIER
Provide a material manufacturer/supplier warranty:
	[~] years
	For the Entrada Horizon Canopy system

	[~] years
	For powder coat finish durability and colour



Provide this warranty on the manufacturer/supplier standard form (if not available then use the standard form in the general section 1237WA WARRANTY AGREEMENT). Commence the warranty from the date of practical completion of the contract works.
Refer to the general section 1237 WARRANTIES for additional requirements.
1.6	WARRANTY - INSTALLER/APPLICATOR
Provide an installer/applicator warranty:
	[~] years
	For installation



Provide this warranty on the installer/applicator standard form (if not available then use the standard form in the general section 1237WA WARRANTY AGREEMENT). Commence the warranty from the date of practical completion of the contract works.
Refer to the general section 1237 WARRANTIES for additional requirements.
REQUIREMENTS
1.7	QUALIFICATIONS - MANUFACTURER/SUPPLIER REQUIREMENTS
Installers to be approved by Entrada. Refer to 1270 CONSTRUCTION for additional requirements relating to qualifications.
1.8	NO SUBSTITUTIONS
Substitutions are not permitted to any of the specified systems, components and associated products listed in this section.
1.9	SHOP DRAWINGS
Refer to the general section 1235 SHOP DRAWINGS for the requirements for submission and review and the provision of final shop drawings.
Provide shop drawings to show the general arrangement including, but not limited to:
1. Overall canopy dimensions
1. Wall bracket and fixing locations
1. Tie rod locations and tie rod wall fixing points
1. Flashing details
1. Sealants and air seals
1. Gutter and downpipe dropper location
1. Non-standard fixing details including brackets
1. Sequence/methodology of installation

If requested provide the following additional information:
1. Provision for the exclusion and/or drainage of moisture
1. Provision for adjustment of fixings to ensure true alignment of the canopy
1. Provision for thermal movement
1. Provision for seismic movement and movement under wind loads
1. Information of Professional Indemnity Insurance held by the person providing the calculations and shop drawings

Submit shop drawings for review to [Name].
[~] working days (at least) before fabrication is planned to commence, provide shop drawings for review. Complete shop drawing review before commencing fabrication.
1.10	INFORMATION FOR OPERATION AND MAINTENANCE
Refer to the general section 1239 OPERATION & MAINTENANCE for provision of operation and maintenance information as electronic PDF format documents:
1. Entrada Care & Maintenance Manual (ENT-CM)

Provide this information prior to practical completion.
1.11	INFORMATION REQUIRED FOR CODE COMPLIANCE
Provide the following compliance documentation:
1. Producer Statement - Construction (PS3) from the installer/applicator
1. Other information required by the BCA in the Building Consent Approval documents
2	PRODUCTS
MATERIALS
2.1	ALUMINIUM
	Sheet
	Grade 5005

	Extrusion
	Grade 6060



Aluminium structures to AS/NZS 1664.1. Aluminium alloys (solid and hollow shapes) to AS/NZS 1866. Aluminium sheets and plates to AS/NZS 1734.
2.2	STEEL
Steel structures to NZS 3404.1 and NZS 3404.2. Cold-formed steel structures to AS/NZS 4600, cold-formed steel sections to AS/NZS 1163. Hot-rolled steel plates to AS/NZS 3678, hot-rolled steel flats to AS/NZS 1594.
CANOPY
2.3	ENTRADA HORIZON CANOPY SYSTEM
Tie rod supported canopy system consisting of:
1. Aluminium canopy tray, powder coat finish
1. Stainless steel tie rod tie-back system
1. Fixings and fixing components
1. Gutter
1. Downpipe dropper
ACCESSORIES
2.4	SEALANT
Sikaflex®-11 FC, a one-component, gun-grade adhesive and sealing compound of permanent elasticity based on a moisture-cured polyurethane.
3	EXECUTION
CONDITIONS
3.1	DELIVERY, STORAGE AND HANDLING OF PRODUCTS
Refer to 1270 CONSTRUCTION for requirements relating to delivery, storage and handling of products.
3.2	ROUTINE MATTERS
Refer to 1250 TEMPORARY WORKS & SERVICES for protection requirements. Refer to 1270 CONSTRUCTION for requirements relating to defective or damaged work, removal of protection and cleaning.
3.3	PRE-INSTALLATION REQUIREMENTS
Check work previously carried out and confirm it is of the required standard for this part of the work.
FABRICATION
3.4	FABRICATION
Fabricate the canopy and associated products as detailed and in accordance with Entrada requirements. Do not cut, drill or modify Horizon components on site except as shown in Entrada installation documentation.
3.5	COLD FORMED
Ensure cold formed work is free from warping, buckling and fractures. Form bends with a brake press or by cold rolling.
3.6	CORNERS
Unless specified otherwise, mitre junctions of identical sections.
3.7	HOLES
Form without distortion of surrounding metal.
3.8	CLEANING DURING ASSEMBLY
Remove all burrs and sharp arrises which would be visible after fixing, or a hazard to the user. Remove any slag or spatter from the welds.
3.9	RIVETED JOINTS
Draw riveted joints tightly together, with rivets closed to completely fill holes.
3.10	MECHANICAL JOINTS
Ensure mechanical joints are tight with no gaps. Use fixings suited to purpose and as specified by Entrada.
3.11	PREPARATION FOR COATINGS
Before applying coatings remove all welding slag, weld spatter, anti-spatter compounds, paints, grease, flux, rust, burrs and sharp arrises. Make good all defects which would show after application of coating. Finish surfaces smooth.
INSTALLATION/APPLICATION
3.12	STANDARDS AND TOLERANCES
Refer to the general section 1270 CONSTRUCTION for general requirements.
3.13	INSTALLATION GENERALLY
Install the canopy system plumb, true to line and face, and square in accordance with Entrada installation documentation and the project-specific engineered design documentation.
Install tie rods and tie rod wall fixings in the locations shown on the shop drawings and in accordance with Entrada installation documentation.
3.14	SEPARATION
Isolate dissimilar materials and dissimilar metals in close proximity by painting the surfaces or fitting separator strips such as high density polyethylene packers.
COMPLETION & COMMISSIONING
3.15	COMPLETION MATTERS
Refer to 1270 CONSTRUCTION for completion requirements and if required commissioning requirements.
4	SELECTIONS
For further details on selections go to entradacanopies.com. Substitutions are not permitted to the following, unless stated otherwise.
CANOPY SYSTEM
4.1	ENTRADA HORIZON CANOPY SYSTEM
	Location
	[Location on drawings]

	Brand
	Entrada Horizon Canopy

	Material
	Aluminium trays / stainless steel tie rods and fasteners

	Size (width × projection)
	[mm × mm]

	Fixing method/type
	[Fixing method/type]

	Finish
	[Powder coat range] powder coat

	Colour
	[Colour name]
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