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1.
True or False? Bulldozer safety starts before you even get behind the wheel.
       
True

       
False

2.
True or False? The best way to inspect a bulldozer for hydraulic fluid leaks is to 

run your fingers over the hydraulic cylinders to check for any moisture.
       
True

       
False

3.
True or False? When you’re operating a bulldozer, wet materials can be harder to 


move than dry materials, especially mud.
       
True

       
False

4.
True or False? “Straight dozing” involves building “walls” around each side of the 


bulldozer’s path.
       
True

       
False

5.
True or False?  When bulldozer operators have limited visibility, they may use a 

“spotter” to help them.
       
True

       
False

6.
True or False? When you’re spotting for a bulldozer operator, you should give them 

your undivided attention to make sure you are as accurate as possible with your 

directions.
      
True

       
False

7.
True or False? Before you operate a bulldozer, you should prepare yourself physically 


by getting a good night's sleep.
       
True

       
False

8.
True or False? A bulldozer’s operator’s manual should be kept in a central area 


where all workers have access to it.
       
True

       
False

9.
True or False? If a bulldozer fails its inspection, you should use extra caution as 


you operate it and notify your supervisor at the end of the day.
       
True

       
False

10.
True or False? Side-by-side dozing requires two dozers.



       
True

       
False
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