Lumen-King Gold Series 1000W LED

The Gold Series 1000W is the most powerful and most efficient fixture Lumen King makes: 3.35 µmol/J efficacy and an enormous PPF of 3350 µmol/s from eight full-spectrum LED bars. It comfortably outperforms double-ended HPS while consuming far less energy.

Full-spectrum output carries plants through every growth stage, from vegetative to flowering, for vigorous, healthy development. The dimmable driver (0-10V signal or knob) gives precise control over intensity, and the Lumen King Eco Controller (sold separately) synchronizes and manages up to 30 fixtures from a single unit.

The foldable eight-bar design installs quickly, spreads light evenly across large canopies to prevent hotspots, and cools passively and silently — no moving parts.

Built to professional standards: full-spectrum output, CE/UKCA/RoHS certification, an IP44 rating and a 2-year warranty.
