**To prevent injury or fire, it is important to maintain good order at the workplace.**

Waste, material residues, packaging, and other combustible items must be removed as soon as possible. Spills of oil or chemicals must be cleaned up immediately. Contractors are responsible for cleaning and tidying up after the work tasks included in their assignment.

**Waste Sorting**

Initially, there will be containers for sorting waste in Hall 45.

* **Combustible:** EPS blocks/Styrofoam, plastic straps, hard plastic, packaging (not corrugated cardboard)
* **Corrugated cardboard**
* **Plastic/LDPE:** Transparent plastic film
* **Sheet waste/Wood:** Single-use pallets, unpainted wood, and chipboard
* **Metal:** Cable trays, metal scrap, screws, etc.
* **Cable scrap:** Cables
* **Hazardous waste:** Waste oil, solvents, absorbents, batteries, fluorescent tubes

If you have any questions, contact your supervisor.

**Red areas on the map are waste stations.**

