# Permit/Checklist for Hot Work at Gyllensvaans Möbler

**All items on the list MUST be checked off before work begins.**

Alarm Address: Gyllensvaans Möbler, Storgatan 6, 52195 Kättilstorp

Work Method: ☐ Welding ☐ Cutting ☐ Soldering

☐ Hot Air ☐ Other: ………………………………………

The permit is valid for today. Date: …………………

## Checklist

☐ I am authorized to perform the work

☐ Person responsible for the work and post-work inspection for 1 hour, Name: …………………

☐ The work area is cleaned and, if necessary, watered

☐ Flammable materials at and near the work area have been removed, covered, or shielded

☐ Heat-conducting structures and hidden flammable building components are protected and accessible for immediate fire extinguishing

☐ Gaps, holes, penetrations, and other openings at and near the work area are sealed or controlled and protected to prevent spark spread

☐ Approved, functional, and sufficient fire extinguishing equipment of the correct type is available for immediate use

☐ If using welding equipment, make sure it’s fault-free. The acetylene cylinder is equipped with a flashback arrestor. The welding torch is equipped with check valves for fuel gas and oxygen. Protective gloves and a shut-off key are available

☐ You have located the nearest fire alarm button so you know where to raise the alarm in case of a fire.

Work approved by supervisor Signature of performer

………………………………………………… ………………………………………………….

Signature Signature

………………………………………………… ………………………………………………….

Name in print Name in print