Railway Regional : Timisoara

Railway Station: CFR Arad

Service Operator : Unicom Tranzit S.A.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Nr. crt** | **Titlu** | **Informaţii generale** | | | | |
| **1. Informaţii generale** | | | | | | |
| **1.1** | Service Facility Operator | Unicom Tranzit SA, with registered office in Voluntari, b-dul Pipera , nr. 1-IA, corp A, etaj 3,4 si 5, jud Ilfov, postal code 077191, tel./fax.021.232.99.48, e-mail: [tranzit@unicom-group.ro,](mailto:tranzit@unicom-group.ro) website: https://unicom-tranzit.ro/ | | | | |
| **1.2** | Validity period and updating process | 01.12.2021 – 30.11.2024 | | | | |
| **2. Services** | | | | | | |
| **2.1** | Name of service no. 1 | Description of service | | Parking/accumulation of freight wagons for formation and dispatch of wagon groups/loading-unloading, in the Arad railway station | | |
| Type of service | | additional | | |
| **3. Description of the Services Facilities** | | | | | | |
| **3.1** | List of Service Facilities | **No.** | **Name** | | | **Supplied Services** |
| **1** | Line 1B | | | 1. Convoy access from/on industrial lines; 2. Wagon parking. |
| **3.2** | Facility No. 1 | Name | | | 1B | |
| Location | | | Arad Railway Station | |
| Opening hours | | | Permanent | |
| Technical  Characteristics | | | Access from line 4C end X through section no. 71 located at km 629+816  Constructive length 813m Actual length 796m  Total leased length 916 ml between km 629+849 and km 630+765 Track material type 49 on concrete sleepers, indirect fastening K  Minimum radius of curves 351m | |
| Planned changes | | | - | |
| **4. Charges** | | | | | | |
| **4.1** | Information on Charges | Not the case. | | | | |
| **4.2** | Information about tariff discounts | Not the case. | | | | |
| **5 Access Conditions** | | | | | | |
| **5.1** | Legal Requirements | The shunting on lines 1B is performed by RU Unicom Tranzit. | | | | |
| **5.2** | Technical Conditions | The shunting is performed by OTF Unicom Tranzit, the maximum speed during the shunting is 30 km/h. | | | | |
| **5.3** | Self-supply of Services | Not the case. | | | | |
| **5.4** | IT Systems | Not the case. | | | | |

|  |  |  |
| --- | --- | --- |
| **6. Allocation of Service Capacity** | | |
| **6.1** | Access Request | Not the case. |
| **6.2** | Response to Request | Not the case. |
| **6.3** | Available Capacity and Temporary Restrictions | Not the case. |